

**PROFILOT**

outbound profiles for eg Arvato-SolarEdge


By giving the 2 profiles the same name, we can have 1 combined POD2Edi setup



Profile for outbound status messages (eg IOC/IOA/IOL/IOD)




Profile for outbound Podlink message on delivery (POD)



**FCD**

Program = MEDIAREF, Field = LAYOUT, SubField = partnername


In Content + text the types of POD are set which are allowed to be transmitted for the partner



|  |  |  |
| --- | --- | --- |
| **DocumentType** | **Description** | **Source** |
| COPAPOD | External POD from 3rd party | EDI |
| EPODPDF | Complete electronic POD | DMP (Mobility) |
| EXTPOD | External POD from partner / weblink | DMP (Mobility) |
| PPOD | Picture POD from PDA | DMP (Mobility) |
| SHORTPOD | Bottom part of electronic POD | DMP (Mobility) |
| SIGNPDA | Signature on PDA | DMP (Mobility) |
| SPOD | Scanned POD | Scanning Station |

**POD2EDI**

Setup to link customer to an outbound profile



For PODlink message to be sent, and the PODlink Image profile to be activated in the righthand bottom corner the Mediaref needs to be filled in with MT(Mediatype) = IMAGE and X in 2nd field